**We shape our buildings: Thereafter, they shape us.**

**JB INDUSTRIES:**

[**JB Industries**](https://jbplaster.in/)**,** Established in the year 1966, An ISO 9001:2008 Company in one of the leading producers of Plaster & Wall putty. The company with an overall experience of Four decades and extensive R&D has been contributing to multi-sectoral needs through its product excellence & technology.

The company has its manufacturing Unit at Hisar with a production capacity of 1.5 Mn TPA. The company has a strong presence & network in north India.

**OUR CORE VALUES:**

**QUALITY:** We are committed to producing the best quality products to match the best standards at reasonable prices.

**ECO-FRIENDLY:** We believe in producing quality products keeping in mind to maintain the eco-balance and ours.

**TRUST:** Over the years our commitment to quality and service we have been able to maintain the trust of ours.

**SERVICE:** Our commitment to being honest & ethical in all our production, market, financial & operational practices.

**JB Plaster Products:**

[**JB Plaster:**](https://jbplaster.in/jb-plaster/)JB Industry is manufacturing JB One Coat plaster (VermiGyp) Our products JB Gypsum Building Plaster & JB One Coat Plaster are available in 20/25 Kg HDPE bags.

[**JB-Wall-Putty**:](https://jbplaster.in/jb-wall-putty/) We, J.B.Industries are manufacturing Plaster of Paris in the name of J.B.Plaster from the year1996 at our Hisar (Haryana) Plant. Now in addition to it, we have started manufacturing a product used for holding the structure of False Ceiling called Hex Bolt Expansion sleeve fastener at our Hisar Plant.

[**JB-Vermigyp:**](https://jbplaster.in/jb-vermigyp/)JB Industry is manufacturing JB One Coat plaster (VermiGyp) Our products JB Gypsum Building Plaster & JB One Coat Plaster are available in 20/25 Kg HDPE bags.Our products JB Gypsum Building Plaster & JB One Coat Plaster are available in 20/25 Kg HDPE bags.

[**JB-Bond:**](https://jbplaster.in/jb-bond/)JB Bond is a bonding agent that provides excellent performance to bond Gypsum Plaster /Sand Cement Plaster on smooth low suction internal RCC surfaces and it eliminates hacking roughening and putting wire mesh on the concrete surface. It is specially formulated for ready to use adhesive consisting of organ resins with additives.

[**JB-Fasteners:**](https://jbplaster.in/jb-fasteners/)We, J.B.Industries are manufacturing Plaster of Paris in the name of J.B.Plaster from the year1996 at our Hisar (Haryana) Plant. Now in addition to it, we have started manufacturing a product used for holding the structure of False Ceiling called Hex Bolt Expansion sleeve fastener at our Hisar Plant.

[**JB-Screws:**](https://jbplaster.in/jb-screws/)J.B. Dry Wall Screw is a specialized Self Tapping Screw. These Screws have a Bugle Head. J.B. Dry Wall Screw can be easily identified by its black finish. This black coloring comes from a phosphate mineral Coating that is applied to these Screws. This coating helps to minimize rusting & corrosion as the Screws are exposed to wet joint compound/Paint.

**Research-Development:**

Continues [**Research and development**](https://jbplaster.in/research-development/) is an integral part of the company’s policy. This has led us to produce one of the best product ranges in the country and meet the needs of the customers. By adopting new technologies & innovation we continue with improvement in existing products and development of new products.

Our R&D team & latest equipment has helped us to meet global standards.

With the best equipment and R&D specialists our aim to continue producing new & innovating products & helping the construction industry grow in India